To comply with the latest Federal (OSHA) regulations to protect workers from exposure to respirable asbestos, silica and other dangerous dust, many handheld power tools must be shrouded and connected to HEPA Vacuums. To maximize dust control without sacrificing efficiency, HEPAPro Vacuums are equipped with a 120V outlet for plugging-in power tools. This outlet allows the operator to use the power tool as the on/off switch for the vacuum. Activate your power tool and your vacuum will turn on. Shut-down your power tool and the vacuum will turn off after seven seconds to allow all the dust to travel the length of the hose to the inside of the tank.
