Synthetic microfiber disposable filter bags trap and contain smaller particles and help extend the life of the HEPA filter. They have greater holding capacity and will not tear or burst even when picking-up heavy concrete dust. The 4-ply construction provides more efficient, extended cleaning periods by providing higher suction and airflow even when the bag is loading. Bottom line, there are fewer interruptions due to clogging, saving you time & money. Also, the bag inlet collar includes a peel-n-stick tab to safely contain the bag’s contents, preventing worker exposure to dangerous dust during transport, handling and disposal.
